**YELLOW GREASE**

Is water resistant multi-purpose calcium grease containing fibers, formulated with good quality base oils and high performance additives. It is recom- mended for low or medium rpm engines equipped with flat or ball bearings where operating temperature not exceeding 110 °C.

***Technical Specifications***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method NLGI 0 NLGI 1 NLGI 2 NLGI 3** |  |
| **Color** | Yellow |  |
| **Soap Type** | ASTM D2270 Calcium |  |
| **Cone Penetration, worked, 0,1 mm, 25 °C /** | ASTM D217 355-385 310-340 265-295 220-250 |  |
| **Dropping Point, °C** | ASTM D566 min 90 min 100 min 100 min 100 |  |