**SLIDE OILS**

SLIDE OIL, is formulated with high quality base oils and quality tackifier additives to enhance the crucial property of adhesion and reduce stick–slip. Used for lubrication of horizontal and vertical slides of all types of machine tools.

***Technical Specifications-32***

|  |  |  |
| --- | --- | --- |
| **Test** | **Method** | **Typical Properties** |
| **Appearance** | Visual | Clear &Bright |
| **Kinematic Viscosity (40°C), [cSt]** | ASTM D445 | 28,8-35,2 |
| **Viscosity Index** | ASTM D2270 | Min. 95 |
| **Flash Point, °C** | ASTM D92 | Min. 205 |
| **Pour Point, °C** | ASTM D97 | Max. -12 |
|  |  |  |